{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["灯具参数明细表"],"not_rendered":{"images":4},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"灯具参数明细表","index":0,"n_rows":12,"n_cols":8,"rows_kept":12,"merged":[[0,0,0,7],[1,0,1,4],[7,0,7,6]],"flags":["formulas_cached_only"]}
["物业升级管理服务之海心沙灯具、灯杆及南广场LED显示屏拆除等零星维修维护项目工程量清单"]
[]
["序号","产品名称","图片","技术要求","数量","单位","综合单价","综合合价"]
[1,"修复星光大道的意大利天工大型投光灯",null,"1.光源：2500W 飞利浦光源            2.输入电压：AC220V                        3.防护等级：IP65                                5.光色：RGB                      6.材质特性：压铸铝主体+不锈钢面盖+背面散热片，钢化玻璃，耐高温硅胶密封圈）                                                     7.整灯功率：2500W                        8.维修项目：更换变压器、风扇与维修控制板，调试正常",6,"盏"]
[2,"P4停车场切割高杆灯杆",null,"1.15米高杆灯杆                  2.用吊车从走道与草地中进行拆除                                                                                     3.风焊割一杆为4节与烧割灯杆头                                4.拆除后运回海心沙仓库",13,"支"]
[3,"拆海心沙风帆下16个天棚灯（高空作业）",null,"1.爬上海心沙4个风帆架，高空拆除16盏天棚灯                          2.使用安全带进行拆除                       3.将拆除灯具运回仓库封存",16,"盏"]
[4,"拆羊城之眼三个大显示屏",null,"1.羊城之眼三块LED大屏屏体、电源、控制器及播控电脑设备等拆除\n2.羊城之眼三块LED大屏屏体铁架风焊割除运回    \n3.羊城之眼三块LED大屏屏体用吊车吊运入东区14栋2单元201室（因门窗楼道狭窄无法搬运，须使用吊车调运）",3,"台"]
["合计"]
[]
[]
[{"$nulls":3},"报价单位：（盖章）"]
[{"$nulls":3},"联系人及联系电话："]