{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["工程量清单"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"工程量清单","index":0,"n_rows":43,"n_cols":9,"rows_kept":43,"merged":[[0,0,0,8],[1,0,1,8],[2,0,3,0],[2,1,3,1],[2,2,3,3],[2,4,3,4],[2,5,3,6],[2,7,2,8],[4,2,4,3],[4,5,4,6],[5,2,5,3],[5,5,5,6],[6,2,6,3],[6,5,6,6],[7,2,7,3],[7,5,7,6],[8,2,8,3],[8,5,8,6],[9,2,9,3],[9,5,9,6],[10,2,10,3],[10,5,10,6],[11,2,11,3],[11,5,11,6],[12,2,12,3],[12,5,12,6],[13,2,13,3],[13,5,13,6],[14,2,14,3],[14,5,14,6],[15,2,15,3],[15,5,15,6],[16,2,16,3],[16,5,16,6],[17,2,17,3],[17,5,17,6],[18,2,18,3],[18,5,18,6],[19,2,19,3],[19,5,19,6],[20,2,20,3],[20,5,20,6],[21,2,21,3],[21,5,21,6],[22,2,22,3],[22,5,22,6],[23,2,23,3],[23,5,23,6],[24,2,24,3],[24,5,24,6],[25,2,25,3],[25,5,25,6],[26,2,26,3],[26,5,26,6],[27,2,27,3],[27,5,27,6],[28,2,28,3],[28,5,28,6],[29,2,29,3],[29,5,29,6],[30,2,30,3],[30,5,30,6],[31,2,31,3],[31,5,31,6],[32,2,32,3],[32,5,32,6],[33,2,33,3],[33,5,33,6],[34,2,34,3],[34,5,34,6],[35,2,35,3],[35,5,35,6],[36,2,36,3],[36,5,36,6],[37,2,37,3],[37,5,37,6],[38,2,38,3],[38,5,38,6],[39,2,39,3],[39,5,39,6],[40,0,40,7],[41,0,41,7],[42,0,42,7]],"flags":["formulas_cached_only"]}
["工程量清单"]
["项目名称：流花展贸中心18号馆水泵房消防泵维修及消防管道改造项目"]
["序号","项目名称","项目特征描述",null,"计量单位","工程量",null,"金额（元）"]
[{"$nulls":7},"综合单价","综合合价"]
[null,"拆除部分"]
[1,"排污泵拆除","1.名称:排污泵\n2.规格、型号:4.5KW\n3.质量:0.5t内",null,"台","2"]
[2,"消防泵拆除","1.名称:消防泵\n2.规格、型号:37KW\n3.质量:1t内",null,"台","2"]
[3,"镀锌钢管拆除 DN150","1.安装部位:室内  \n2.输送介质:给水  \n3.材质:镀锌钢管  \n4.型号、规格:DN150mm  \n5.连接方式:卡箍连接 \n6.管道刷油:防锈漆两遍、调和漆两遍",null,"m","51"]
[4,"闸阀拆除 DN150","1.类型：闸阀\n2.材质：铸钢\n3.规格、型号：DN150\n4.连接形式：法兰连接",null,"个","4"]
[5,"止回阀拆除 DN150","1.类型：止回阀\n2.材质：铸钢\n3.规格、型号：DN150\n4.连接形式：法兰连接",null,"个","4"]
[6,"软接头(软管)拆除 DN150","1.类型：橡胶软接头\n2.材质：橡胶\n3.规格、型号：DN150\n4.连接形式：法兰连接",null,"个","4"]
[null,"电气部分"]
[7,"配电箱","1.名称:排污泵配电箱\n2.规格、型号:半周长1.5米内\n3.安装方式:挂墙明装",null,"台","1"]
[8,"镀锌线槽","1.名称:镀锌线槽\n2.材质:碳钢\n3.规格:50*50",null,"m","4"]
[9,"配线","1.名称:电线敷设\n2.配线形式:线槽配线\n3.规格、型号:NH-BV-2.5mm",null,"m","120"]
[10,"配线","1.名称:电线敷设\n2.配线形式:线槽配线\n3.规格、型号:NH-BV-4mm",null,"m","100"]
[11,"低压交流异步电动机","1.名称:电机接线检查\n2.容量(kW):4.5KW",null,"台","2"]
[12,"低压交流异步电动机","1.名称:电机接线检查\n2.容量(kW):37KW",null,"台","2"]
[null,"给水部分"]
[13,"原排污泵安装","1.名称:排污泵\n2.规格、型号:4.5KW\n3.质量:0.1t内",null,"台","2"]
[14,"原消防泵安装","1.名称:消防泵\n2.规格、型号:37KW\n3.质量:1t内",null,"台","2"]
[15,"镀锌钢管","1.安装部位:室内  \n2.输送介质:给水  \n3.材质:镀锌钢管  \n4.型号、规格:DN20mm  \n5.连接方式:螺纹连接 \n6.管道刷油:防锈漆两遍、调和漆两遍",null,"m","16"]
[16,"镀锌钢管","1.安装部位:室内  \n2.输送介质:给水  \n3.材质:镀锌钢管  \n4.型号、规格:DN80mm  \n5.连接方式:螺纹连接 \n6.管道刷油:防锈漆两遍、调和漆两遍",null,"m","21"]
[17,"镀锌钢管","1.安装部位:室内  \n2.输送介质:给水  \n3.材质:镀锌钢管  \n4.型号、规格:DN100mm  \n5.连接方式:卡箍连接 \n6.管道刷油:防锈漆两遍、调和漆两遍",null,"m","20"]
[18,"原镀锌钢管重新安装","1.安装部位:室内  \n2.输送介质:给水  \n3.材质:镀锌钢管  \n4.型号、规格:DN150mm  \n5.连接方式:卡箍连接 \n6.管道刷油:防锈漆两遍、调和漆两遍",null,"m","48"]
[19,"螺纹截止阀 DN15","1.类型:截止阀\n2.材质:铜质\n3.规格、压力等级:DN15 1.6MPa\n4.连接形式:螺纹连接",null,"个","4"]
[20,"螺纹截止阀 DN50","1.类型:截止阀\n2.材质:铜质\n3.规格、压力等级:DN50 1.6MPa\n4.连接形式:螺纹连接",null,"个","2"]
[21,"螺纹阀门","1.类型:止回阀\n2.材质:铜质\n3.规格、压力等级:DN50 1.6MPa\n4.连接形式:螺纹连接",null,"个","2"]
[22,"法兰闸阀","1.类型:闸阀\n2.材质:铸钢\n3.规格、压力等级:DN100 1.6MPa\n4.连接形式:法兰连接",null,"个","2"]
[23,"法兰泄压阀","1.类型:泄压阀\n2.材质:铸钢\n3.规格、压力等级:DN100 1.6MPa\n4.连接形式:法兰连接",null,"个","2"]
[24,"液压浮球控制阀","1.类型:液压浮球控制阀\n2.材质:铸钢\n3.规格、压力等级:DN100 1.6MPa\n4.连接形式:法兰连接",null,"个","2"]
[25,"法兰闸阀","1.类型:闸阀\n2.材质:铸钢\n3.规格、压力等级:DN150 1.6MPa\n4.连接形式:法兰连接",null,"个","2"]
[26,"原法兰闸阀","1.类型:闸阀\n2.材质:铸钢\n3.规格、压力等级:DN150 1.6MPa\n4.连接形式:法兰连接",null,"个","4"]
[27,"原法兰止回阀","1.类型:止回阀\n2.材质:铸钢\n3.规格、压力等级:DN150 1.6MPa\n4.连接形式:法兰连接",null,"个","4"]
[28,"原软接头(软管)","1.类型：橡胶软接头\n2.材质：橡胶\n3.规格、型号：DN150\n4.连接形式：法兰连接",null,"个","4"]
[29,"报警装置","1.名称：湿式报警阀\n2.型号、规格：DN150",null,"组","1"]
[30,"压力仪表","1.名称:压力表\n2.规格:2.5MPa",null,"块","4"]
[31,"管道支架","1.形式:吊托支架 \n2.材质:碳钢(型钢综合) \n3.除锈、刷油:人工除锈两遍、刷红丹两遍、刷调和漆两遍",null,"kg","119.34"]
[null,"措施项目"]
[32,"脚手架搭拆",null,null,"项","1"]
["小   计"]
["税费（10%）"]
["合   计"]