{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["工程量"],"not_rendered":{"images":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"工程量","index":0,"n_rows":10,"n_cols":9,"rows_kept":10,"merged":[[0,0,0,8],[3,1,3,7],[4,1,4,7],[5,1,5,7]],"flags":["formulas_cached_only"]}
["海心沙看台轮廓灯修复工程量报价表"]
["序号","产品名称","图片","技术要求","维修内容","单位","数量","不含税单价","不含税合价"]
[1,"LED 数码管(L3)",null,"1.光源：720*0.06W 晶科芯片                 2.输入电压：DC24V  DMX-512控制                            3.型号：JM06-307201RGB\n4.防护等级：IP65                  5.尺寸：原灯体                     6.光色：RGB                       7.材质特性：拉伸铝灯体，钢化玻璃，耐高温硅胶密封圈）                8.整灯功率：45W","1.拆除原有LED灯具；\n2.LED灯板（线路板）更换为5050RGB灯珠；\n3.恒压电源更换；\n4.更换新的DMX512控制板；\n5.安装LED灯具；\n6.调试","套","43"]
[2,"不含税费用合计"]
[3,"税费（税率  %）"]
[4,"含税费总价"]
[]
[]
[{"$nulls":4},"报价单位：（盖章）"]
[{"$nulls":4},"联系人及联系电话："]