{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":17,"n_cols":4,"rows_kept":17,"merged":[[0,0,0,3],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3]],"flags":["formulas_cached_only"]}
["流花展贸中心北区空调主机房集水井盖板整改项目\n工 程 量清单"]
["序号 ","分项目名称","单位","数量"]
[]
["一","北区空调主机房挖沉池"]
[1,"挖沉池（风炮打混泥土）1米*1米*1米","M3  ",2]
[2,"清挖余泥（工人装袋从负一楼搬上一楼）","M3  ",2]
[3,"堵漏剂","㎡",10]
[4,"砌砖挡土墙（18㎝厚）（红砖）","㎡",8]
[5,"地面植筋与池边相连","根",100]
[6,"扎钢筋（100根10里）及钉模板","㎡",10]
[7,"倒混泥土","M3  ",10]
[8,"做黑豹涂膜防水(做三次）","㎡",10]
[9,"铺电线（2.5平方)及装控制箱(配置一主一备)（控制箱订做）","个",2]
[10,"铺水管(联塑PVC75)","m",8]
[11,"安装清水泵","台",2]
[12,"沉箱盖(镀锌)","个",2]
[13,"余泥清运费(157公里右左)","车",1]