{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":17,"n_cols":5,"rows_kept":17,"merged":[[0,0,0,4],[1,0,1,3]],"flags":["formulas_cached_only"]}
["流花展贸中心招商中心搬迁项目                                                "]
["工程名称：建隆办公室零散维修"]
["序号","项  目  名  称","数量","单位","备  注"]
[1,"铲除旧墙面，墙面油漆翻新(、刮腻子粉、打磨上油漆3遍)",146.5,"m2","铲除旧墙面、刮腻子粉.立邦油漆"]
[2,"拆除旧石膏板天花",3.8,"m2","拆除原有破损天花、清走"]
[3,"开关移位(3位)",1,"个","原有开关移位至新砌墙接近位置"]
[4,"墙面开洞",1,"个","人工开工、清走淤泥"]
[5,"安装排气扇,12寸",1,"把","根据现场实际情况安装排气扇"]
[6,"拆除玻璃面广告纸",33.6,"m","玻璃面广告纸拆除"]
[7,"拆除旧大理石收银台",3,"m3","拆除、清走"]
[8,"新砌20cm厚砖墙",14.1,"m2","蒸压加气砖、混水墙、20cm厚度"]
[9,"新砌墙面批荡",28.2,"m2","1:2水泥砂浆15mm厚度基层1:2.5水泥砂浆5mm厚度面层"]
[10,"水泥砂浆找平",12.7,"m2","1：2.5水泥砂浆5cm厚度找平"]
[11,"新铺瓷片",12.7,"m2","与原地转接近颜色，700*700"]
[12,"复原嵌入式筒灯",16,"盏","3.5寸9w白色砂银材质"]
[13,"嵌入式led灯盘",2,"个","600*600、28瓦双驱进口"]
[14,"新做硅钙板吊顶",28.6,"m2","6mm厚度硅钙板轻钢龙骨吊顶"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}