{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["工程量"],"read":"whole","date_system":"1900"}

{"sheet":"工程量","index":0,"n_rows":38,"n_cols":7,"rows_kept":38,"merged":[[0,0,0,6],[33,1,33,5]]}
["海心沙宿舍及亚运公园零星维修项目工程量清单"]
["序号","项目名称","项目特征描述","计量单位","工程量","单价","合价"]
[null,"海心沙宿舍"]
[1,"铲除墙面腻子及油漆","铲除墙面腻子及油漆","m2",76]
[2,"铲除天棚腻子及油漆","铲除天棚腻子及油漆","m2",30]
[3,"抹灰面油漆","刮腻子二遍， 乳胶漆底油二遍面油二遍 墙柱面","m2",76]
[4,"抹灰面油漆","刮腻子二遍， 乳胶漆底油二遍面油二遍 天棚面","m2",30]
[5,"隔墙","轻钢龙骨隔墙，胶合板基层 9mm，饰面层埃特墙板","m2",15]
[null,"风机房通风口"]
[6,"铝合金百叶窗","铝合金百叶窗","m2",3.6]
[null,"人防门"]
[7,"铲除墙面腻子及油漆","铲除墙面腻子及油漆","m2",52]
[8,"抹灰面油漆","刮腻子二遍， 乳胶漆底油二遍面油二遍 墙柱面","m2",52]
[null,"措施项目"]
[9,"天棚活动脚手架",null,"m2",30]
[10,"墙面活动脚手架",null,"m2",128]
[null,"舞台水池喷泉管道外观翻新"]
[11,"人工打磨主管道锈迹及原来油漆面 管径250","人工打磨主管道锈迹及原来油漆面 管径250","m2",196.25]
[12,"人工打磨喷泉管道锈迹及原来油漆面 管径65","人工打磨喷泉管道锈迹及原来油漆面 管径65","m2",61.23]
[13,"人工涂刷主管道  五羊牌防锈漆  管径250","人工涂刷主管道  五羊牌防锈漆  管径250","m2",196.25]
[14,"人工涂刷喷泉管道 五羊牌防锈漆  管径65","人工涂刷喷泉管道 五羊牌防锈漆  管径65","m2",61.23]
[null,"广场不锈钢栏杆焊接"]
[15,"脱焊断裂 变形修复","脱焊断裂 变形修复","m",300]
[null,"地面粘贴反光警示带"]
[16,"地面突出位置贴反光警示带","地面突出位置贴反光警示带","m",60]
[null,"海心沙室外电梯护栏改造"]
[17,"机械拆除不锈钢护栏","机械拆除不锈钢护栏","m",5]
[18,"安装8厚钢化玻璃护栏","安装8厚钢化玻璃","m2",2]
[null,"海心沙室内电梯护栏改造"]
[19,"机械拆除不锈钢护栏","机械拆除不锈钢护栏","m",5]
[20,"安装新不锈钢护栏","更换安装新不锈钢栏杆","m",5]
[null,"拆除看台悬挑木板"]
[21,"搭架拆除看台悬挑木板  3.5米高","搭架拆除看台悬挑木板  3.5米高","m2",300]
[null,"总计"]
[]
[]
[null,null,"报价单位：（盖章）"]
[null,null,"联系人及联系电话："]