{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["清单"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"清单","index":0,"n_rows":26,"n_cols":8,"rows_kept":26,"merged":[[0,0,0,7],[2,0,14,0],[15,0,21,0],[22,0,22,5]],"flags":["formulas_cached_only"]}
["花城汇潜污泵排水系统改造项目工程量清单"]
["位置","项目名称","项目特征","单位","数量 ","单价","合价","备注 "]
["37号泵房","自吸无堵塞排污泵 (卧式泵）","1.拆除原有排污泵； 2.排污泵，流量65m3/h,扬程25m，功率7.5kw，铸铁材质80ZW65-25-7.5      3.安装；                4.调试       ","台",1,null,null,"原格兰富泵：流量60m3/h，扬程28m，功率3.7kw"]
[null,"闸阀","1.闸阀；               2.规格DN100；                 3.安装","个",2]
[null,"止回阀","1.止回阀；               2.规格DN100；           3.安装","个",1]
[null,"软接","1.可曲挠橡胶软接头\n2.规格:DN100\n3.安装","个",2]
[null,"接头","DN100","个",2]
[null,"法兰","DN100","个",1]
[null,"排水管","1.镀锌钢管；          2.规格DN100","m",12]
[null,"自动搅匀潜污泵","1.拆除原有潜污泵；   2.潜污泵，Q=65m3/h，H=25m，7.5kw，铸铁材质，80JYWQ65-25-7.5   3.安装；                  4.调试         ","台",1,null,null,"原格兰富泵：流量19L/S，扬程25m，功率3.7kw)"]
[null,"耦合装置","含耦合器、导轨、拉链","套",1]
[null,"泵坑隔渣设备","不锈钢材质","套",1]
[null,"闸阀","1.闸阀；               2.规格DN100；                 3.安装","个",1]
[null,"止回阀","1.止回阀；               2.规格DN100；           3.安装","个","1"]
[null,"软接","1.可曲挠橡胶软接头\n2.规格:DN100\n3.安装","个",1]
["海印卸货区","自动搅匀潜污泵","1.拆除原有潜污泵；           2.潜污泵，Q=15m3/h，H=25m，2.2kw，304不锈钢材质50JYWQ15-25-2.2 ；                        3.安装；                     4.调试","台",1,null,null,"原格兰富泵：流量4L/S，扬程12m，功率1.5kw"]
[null,"耦合装置","含耦合器、导轨、拉链","套",1]
[null,"泵坑隔渣设备","不锈钢材质","套",1]
[null,"闸阀","1.闸阀；               2.规格DN100；                 3.安装","个",1]
[null,"止回阀","1.止回阀；               2.规格DN100；           3.安装","个",1]
[null,"软接","1.可曲挠橡胶软接头\n2.规格:DN100\n3.安装","个",1]
[null,"排水管","1.镀锌钢管；          2.规格DN100","m",6]
["总  计"]
[]
[{"$nulls":3},"报价单位：（盖章）"]
[{"$nulls":3},"联系人及联系电话："]