{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":8,"n_cols":7,"rows_kept":8,"merged":[[0,0,0,6],[4,1,4,5]],"flags":["formulas_cached_only"]}
["花城汇北区玻璃门及卷闸门维修项目工程量清单"]
["序号","项目名称","项目特征","计量单位","工程量","单价","合价"]
[1,"北区玻璃门维修","1.将门框支撑柱掏空水泥地面                           2.切除原门框支撑柱生锈底部                                 3.切除原门边不锈钢修边                      4.用6厘厚四方槽钢进行切割焊接加固                                                            5.用新不锈钢包边修复                                 6.补填水泥砂浆顿足不平地面                                          7.恢复地面砖，新贴                                8.对损散大门进行全面加槽钢固定，外修饰不锈钢件加固                                         9.损坏门套点焊加固                                          10.对焊点进行打磨、平整外观                                      11.对损坏修复门边、门框打玻璃胶                                                   12.更换不锈钢长拉手                                                                                                                               ","套",54]
[2,"卷闸门维修","1.更换卷闸门电机                                       2.新买卷闸门遥控器                                 3.修复损坏无法打开的自动升降卷闸门，更换控制器                       4.自动卷闸门马达修理                             5.将卷闸门损坏的卷闸门边条更换与维修   ","套",3]
[null,"总计"]
[]
[{"$nulls":3},"报价单位：（盖章）"]
[{"$nulls":3},"联系人及联系电话："]