{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["报价单 "],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"报价单 ","index":0,"n_rows":13,"n_cols":7,"rows_kept":13,"merged":[[0,0,0,6],[9,0,9,5]],"flags":["formulas_cached_only"]}
["物业升级管理服务之花城广场（南广场）监控系统维修项目工程量清单"]
["序号","项目名称","项目特征描述","计量单位","工程量","单价","合价"]
[1,"光线","1.名称：4芯单模铠装光缆（电信级）\n2.中心管式轻铠装","m",500]
[2,"电源线","1.名称：室外防水专用屏蔽电源线缆\n2.规格型号：RVV2*1.0mm2（国标）","m",500]
[3,"视频线","1.名称：75欧辐射频同轴线\n2.规格型号：SYU-75-5 96网编（国标）","m",500]
[4,"信号控制线","1.产品型号：485信号控制线\n2.导体电阻：24*0.185mm/20°C直流电阻：≤26Ω/km","m",500]
[5,"线管","1.名称：联塑PVC线管\n2.规格型号：305（B)型绝缘阻燃","m",700]
[6,"线管辅材","1.管码\n2.座盒\n3.直通","批",1]
[7,"凿（压）槽","1.名称：水泥地及泥地开挖及恢复","m",400]
["总计"]
[]
[{"$nulls":3},"报价单位：（盖章）"]
[{"$nulls":3},"联系人及联系电话："]